|  |  |  |
| --- | --- | --- |
| WORLD METEOROLOGICAL ORGANIZATIONCOMMISSION FOR BASIC SYSTEMS-----------------------------FIRST MEETING OF INTER-PROGRAMME EXPERT TEAM ONDATA REPRESENTATION MAINTENANCE AND MONITORINGTOKYO, JAPAN, 1 - 5 JULY 2013 |  | IPET-DRMM-I / Doc. 3.2 (3)(14.VI.2013)-------------------------ITEM 3.2ENGLISH ONLY |

**New flag table entries in BUFR Table B**

*Submitted by J. Ator (USA)*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Summary and Purpose of Document**

This document proposes two new entries in the flag table for BUFR descriptor 0-33-032.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**ACTION PROPOSED**

The meeting is requested to review the proposed new entries and approve them for pre-operational implementation.

**DISCUSSION**

We request the use of the following unassigned bits in the flag table for BUFR descriptor 0-33-032. We believe that these entries are trivial enough that they should not require a full validation procedure; however, we are happy to undertake that if there is any objection from the meeting. In that case we would ask for volunteers to assist with the validation.

**PROPOSAL**

**Add new flag table entries to 0-33-032 (Channel quality flags for ATOVS)**

7 Quality for this scan is reduced

 8 Pixel is affected by radio frequency interference